# Single Board Computer

***Full-size***

***w w w . i ei w or l d .c om***

**PCIE-H810**

***Full-size PICMG 1.3 CPU card supports LGA 1150 Intel® Core™ i7/i5/i3, Pentium® and Celeron® with Intel® H81, DDR3, VGA, iDP, Dual PCIe GbE, SATA 6Gb/s, mSATA, USB 3.1 Gen 1 (5Gb/s), RS-232, HD Audio and RoHS***

Dual-channel DDR3

2 x SATA 3Gb/s LPT

USB 2.0

1600/1333 MHz

2 x SATA 6Gb/s

2 x USB 3.1 Gen 1

Front panel KB/MS

## Enhanced component protection

Prevent the damage of bottom components

2 x RS-232

USB 2.0 RS-422/485

### LGA 1150

**Intel® H81**

DIO

TPM

PCIe Mini & mSATA colay iDP

LAN

VGA

## PCIe Mini & mSATA colay

The PCIe Mini interface provides PCIe x1, USB and mSATA signal for full-size or half-size PCIe Mini devices, such as SSD, mSATA and wireless LAN cards.

2 x USB 2.0

◄ mSATA

TPM 1.2 Support

# *Features*

DDR3

1600

***USB***

USB 3.1 SATA 6Gb/s PCIe GbE

mSATA

iDP

* PICMG 1.3 full-size solution

▲ Half-size wireless LAN card

# *Specifications*

PCIE-H810-2019-V10

CPU

4th generation LGA 1150 Intel® Core™ i7/i5/i3, Pentium® or Celeron® processor supported Chipset

Intel® H81

Memory

Two 240-pin 1600/1333 MHz dual-channel unbuffered DDR3 & DDR3L SDRAM DIMMs support up to 16 GB

BIOS UEFI

Graphics Engine

Intel® HD Graphics Gen 7.5 supports DX11.1, OpenCL 1.2 and OpenGL 3.2 Full MPEG2, VC1, AVC Decode

Display Output

Dual independent display

1 x VGA (up to 1920x1200@60 Hz)

1 x iDP interface for HDMI, LVDS, VGA, DVI, DP (up to 3840x2160@60 Hz) Ethernet

Dual Realtek RTL8111E PCIe GbE controllers supported

External I/O Interface 2 x USB 2.0

Internal I/O Interface

1 x KB/MS (1x6 pin) 2 x SATA 3Gb/s (AHCI supported, no RAID)

1 x LPT (2x13 pin) 2 x SATA 6Gb/s

1 x RS-422/485 (1x4 pin, P=2.0) 2 x USB 3.1 Gen 1 (5Gb/s) (2x10 pin)

1 x USB 2.0 (180° Type-A) 4 x USB 2.0 (Golden finger)

2 x RS-232 (2x5 pin, P=2.54) 4 x USB 2.0 (2x4 pin, P=2.54)

Audio

Support 7.1-channel HD Audio by IEI AC-KIT-892HD kit Front Panel

1. x Front panel (2x7 pin, power LED, HDD LED, speaker, power button, reset button)

LAN LED

1. x LAN LED (1x2 pin) SMBus

1 x SMBus (1x4 pin)

I²C

1 x I²C (1x4 pin) Infrared Interface

1 x Infrared Interface (1x5 pin)

Expansion

1 x Full/Half-size PCIe Mini slot (supports mSATA) One PCIe x16 & four PCIe x1 signal via golden finger Watchdog Timer

Software programmable supports 1~255 sec. system reset

Digital I/O

8-bit digital I/O (2x5 pin) Fan Connector

1 x CPU smart fan (1x4 pin)

1 x System smart fan (1x3 pin) Power Supply

5V/12V, AT/ATX support

Power Consumption

5V@3.41A, 12V@0.35A, Vcore\_12V@7.52A, 3.3V@1.41A, 5VSB@0.12A

(Intel® Core™ i7-4770K 3.90 GHz CPU with 8 GB (two 4 GB) 1333 MHz DDR3 memory) Operating Temperature: -20°C ~ 60°C

Storage Temperature: -30°C ~ 70°C

Operating Humidity: 5% ~ 95%, non-condensing

Dimensions: 338 mm x 126 mm Weight: GW: 1000g / NW: 420g CE/FCC compliant

* 4th generation LGA 1150 Intel® Core™ i7/i5/i3, Pentium® or Celeron® processor supported
* Two 1600/1333 MHz DDR3 SDRAM DIMMs support up to 16 GB
* Dual Realtek PCIe GbE supported
* TPM v1.2 hardware security function supported by TPM module
* IEI One Key Recovery solution allows you to create raipd OS backup and recovery
* Stiffener bars
* IEI jumper-less function

# *Packing List*

|  |
| --- |
| 1 x PCIE-H810 single board computer |
| 2 x SATA cable |
| 1 x QIG |

***Ordering Information***

|  |  |
| --- | --- |
| Part No. | Description |
| PCIE-H810-R10 | Full-size PICMG 1.3 CPU Card supports LGA 1150 Intel® Core™ i7/i5/i3, Pentium® and Celeron® CPU with Intel® H81, DDR3, VGA, iDP, dual PCIe GbE, SATA 6Gb/s, mSATA, RS-232,USB 3.1 Gen 1 (5Gb/s), HD Audio and RoHS |
| 19800-000049-RS | LPT flat cable, 240mm, P=2.54 |
| 19800-000075-RS | PS/2 KB/MS cable with bracket, 220mm, P=2.0 |
| 19800-003100-300-RS | Dual port USB 2.0 cable with bracket, 300mm, P=2.54 |
| 19800-010500-200-RS | USB 3.1 Gen 1 (5Gb/s) cable with bracket, 450mm |
| 32102-000100-200-RS | SATA power cable, MOLEX 5264-4P to SATA15P |
| 32205-000702-100-RS | RS-232 cable, 230mm, P=2.54 |
| 32205-003800-300-RS | RS-422/485 cable, 200mm, P=2.0 |
| AC-KIT-892HD-R10 | 7.1-channel HD Audio kit with Realtek ALC892 supports dual audio streams |
| CF-1150SB-R11 | Special cooler kit for LGA 1150, high-performance compatible, 65W |
| CF-1150SC-R20 | Special cooler kit for LGA 1150, 1U chassis compatible, 65W |
| CF-1150SE-R11 | Special cooler kit for LGA 1150, high-performance compatible, 95W |
| CF-1150SF-R10 | Special cooler kit for LGA 1150, high-performance compatible, 54W |
| DP-DP-R10 | DisplayPort to DisplayPort converter board (for IEI iDP connector) |
| DP-DVI-R10 | DisplayPort to DVI-D converter board (for IEI iDP connector) |
| DP-HDMI-R10 | DisplayPort to HDMI converter board (for IEI iDP connector) |
| DP-LVDS-R10 | DisplayPort to LVDS converter board (for IEI iDP connector) |
| DP-VGA-R10 | DisplayPort to VGA converter board (for IEI iDP connector) |
| TPM-IN01-R20 | 20-pin Infineon TPM module, software management tool, firmware v3.17 |