

***单板计算机***

***工业主板***




***w w w . i e i w o r l d . c o m***

***ATX主板支持14nmLGA1151Intel®第8代Core™i7 / i5 / i3，Celeron®和Pemtium®处理*** IMBA-Q370 ***器，DDR4，三重独立显示器，双GbE LAN，M.2，USB 3.1 Gen 2（10Gb / s），SATA***

***6Gb / s，HD Audio和RoHS***



|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | 双通道DDR4 2666MHz | |  |  |  | M.2 A key | | | | | | | | | | | | | | | | | | | |  |  |  |  | 机箱 | | |  |
|  |  |  |  | USB 3.1 Gen1 | |  |  |  |  |  |  | 6 x SATA 6Gb/s | | | | | | | | | | | | | | | | |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | Intrusion | | |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 前面板l | | |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | M.2 M key | | |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | RS-232/422/485 | | | | |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | TPM | | |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | RS-232 | | |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 4 x USB 2.0 | | | | | |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 2 x PCI | | |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  | |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Displayport | | | | | |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | LPT (可选) | | |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| KB/MS | | | | | |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  | 前置音频 |  |  |  |  |  |  |  |  | PCIe x8 | | | | | | | |  | DIO | | | | | |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| ***规格*** | | | | | |  |  |  |  |  |  | PCIe x4 2 x PCIe x4 | | | | | | | | | | | | | | | | |  |  |  |  |  |  |  |  |
| PCIe x8 | | | | | | | | | | | | | | | | | | | | | | |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |



 CPU

LGA1151 插槽 支持 8th代 Intel® Core™ i7/i5/i3, Pentium® or Celeron® 处理器 芯片组

Intel® Q370

 BIOS: AMI UEFI BIOS

内存

四个288-pin 2666/2400 MHz 双通道 DDR4 SDRAM 无缓冲 DIMMs 最高支持达64GB

图形引擎

英特尔®高清显卡Gen9引擎具有低功耗16执行单元，支持DX11.3 / 12，OpenGL 4.3 / 4.4 / 4.5和OpenCL1.2 / 2.0 / 2.1

显示输出

三重独立显示

1 x VGA (最高至 1920 x 1080@60Hz)

1 x DP++ (最高至 4096 x 2304@60Hz)

1 x HDMI (最高至 4096 x 2304@30Hz)

1 x 内置 Displayport (最高至 4096 x 2304@60Hz)

 网络

LAN1 : Intel® I219LM PCIe 控制器支持 AMT 11.0

|  |  |  |  |
| --- | --- | --- | --- |
| LAN2: Intel® I211AT PCIe 控制器 | | |  |
| 超级 I/O: 嵌入式控制器 | | |  |
| 外部 I/O 接口 | |  |  |
| 2 x USB 3.1 | Gen 2 | (10Gb/s) | 1 x RS-232 |
| 2 x USB 3.1 | Gen 1 | (5Gb/s) | 1 x PS/2 KB/MS |
| 2 x USB 2.0 |  |  |  |
| 内部 I/O 接口 | |  |  |
| 1 x 180º Displyport | |  | 1 x KB/MS (1x6 pin) |
| 2 x RS-232/422/485 (2x5 pin, P=2.54) | | | 3 x RS-232 (2x5 pin, P=2.54) |
| 2 x USB 3.1 | Gen 1 | (5Gb/s) (2x10 pin, P=2.0) | 4 x USB 2.0 (2x4 pin, P=2.54) |



6 x SATA 6G/s (RAID 0/1/5/10 supported)

 SMBus: 1 x SMBus (1x4 pin)

 I²C: 1 x I²C (1x4 pin)

 音频

Realtek ALC662 高清编解码器

3 x 音频插孔 ( 音频输入 ，音频输出 , 麦克风输入 ）

1 x 模拟音频 (2x5 pin)

 前面板

1 x前面板 (2x7 pin, power LED, HDD LED, 扬声器 , 电源按钮 , 重启按钮 )

 网络灯: 2 x 网络灯 (1x2 pin)

 扩展接口

2 x PCIe x8 1 x M.2 A key (2230, PCIe x1 & USB 2.0)

3 x PCIe x4 1 x M.2 M Key (2280, PCIe x2 only)

2 x PCI

 数字 I/O: 1 x 8-bit 数字 I/O (2x5 pin)

 TPM: 1 x TPM (2x10 pin)

 风扇接口

1 x CPU 风扇接口(1x4 pin)

2 x System 风扇接口 (1x3 pin)

 机箱 : 1 x Chassis intrusion (1x2 pin)

 电源

支持 ATX/AT 电源

支持AT/ATX 模式

ErP/EuP 兼容

 看门狗定时器 : 软件可编程并支持 1~255 秒系统复位

功耗

3.3V@1.65A, 5V@3.4A, 12V@8.58A, 5VSV@3.4A (Intel® Core® i7-8700K up to

4.60 GHz CPU 及 32GB 2600MHz DDR4内存)

操作温度: -20°C ~ 60°C

存储温度: -30°C ~ 70°C



存储湿度 5% ~ 95%, non-condensing

尺寸: 244mm x 305mm

重量: GW:1200g / NW:700g

CE/FCC 标准

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  | **M.2 M key** | | | | | | |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | **M.2 A key** | | | | |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| KB/MS DP++ | | | | | | | | | | | |  |  | RS-232 | |  | LAN1 LAN2 | | | | | | |  |  |  | 音频 | | |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  | |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | |  | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 2 x USB 3.1 Gen 1 | | | | | | | | | | |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  | HDMI | | |  |  |  |  | 2 x USB 3.1 | | | | | |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 2 x USB 2.0 | | | | | | | | | | | |  |  | VGA | |  | Gen 2 | | | | | | |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  | **DDR4** | | | | | | | | |  | **Triple** | | |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **2666** | | | | | | | |  |  |  |  | **Display** | | | |  |  | **DP++** | | | | | |  |  |  | **M.2** | | | **SATA 6Gb/s PCIe GbE** | | | | |  |




***特征***

* 第8代LGA1151英特尔®酷睿™i7 / i5 / i3，赛扬®和奔腾®处理器
* 双通道DDR4 2666MHz
* 支持 VGA, HDMI & DP++
* 支持 M.2 A key for WLAN 扩展, M key 存储
* IEI 一键恢复解决方案可快速创建 OS 备份和恢复


***包装清单***

|  |  |
| --- | --- |
| 1 x IMBA-Q370 single board computer | 2 x SATA cable |
| 1 x I/O shielding | 1 x QIG |
|  |  |

***尺寸*** *(Unit: mm)*



***订购信息***



|  |  |  |
| --- | --- | --- |
| 料号. | 描述 |  |
|  |  |  |
|  | ATX motherboard supports 14nm LGA1151 Intel® 8th |  |
| IMBA-Q370-R10 | Generation Core™ i7/i5/i3, Celeron® and Pemtium® |  |
| processor, DDR4, triple independent displays, dual GbE LAN, |  |
|  |  |
|  | M.2, USB 3.1, SATA 6Gb/s, HD Audio and RoHS |  |
| 19800-000075-RS | PS/2 KB/MS cable with bracket, 220mm, P=2.0 |  |
| 19800-003100-100-RS | Dual port USB cable with bracket, 30mm, P=2.54 |  |
| 19800-010500-200-RS | USB 3.1 Gen 1 (5Gb/s) cable 457mm with bracket |  |
| 32102-000100-200-RS | SATA power cable, MOLEX 5264-4P to SATA15P |  |
| 32205-000702-100-RS | RS-232 cable, 230mm, P=2.54 |  |
| CF1156A-RS-R11 | High-performance LGA1155/1156 cooler kit, 1U chassis |  |
| compatible 73W |  |
|  |  |
| CF-1156C-RS | LGA1155/LGA1156 cooler kit, 1U chassis compatible, 45W |  |
| CF-1156D-RS | LGA1155/LGA1156 cooler kit, 1U chassis compatible, 65W |  |
| CF-1156E-R11 | High-performance LGA1155/1156 cooler kit, 95W |  |
| TPM-IN02-R20 | 20-pin Infineon TPM 2.0 module, software management tool, |  |
| firmware v5. |  |
|  |  |
|  |  |  |



**IMBA-Q370-2019-V10**