

*工业电脑机箱*



*w w w . i e i w o r l d . c o m . c n*




RACK-360G 4U 14个插槽全长卡 机架式机箱


|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 12 cm Fan | | 3.5” FDD | | |  |
|  |  | Filter | Card Clamp | |  |
|  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |



|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  | 5.25”或 |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  | 3.5”驱动器 |  | RACK-360GW | |  | RACK-360GB | | | |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  | 2 x 5.25” |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  | Shock Absorber | | |  |  |
|  |  |  |  |  |  |  |  |  |  | Drive Bay |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | Hold-down Clamp | |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  | 2 x USB | | |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | HDD LED | | | |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 电源 LED | | | | |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  | 电源开关 | | |  | 灵活的驱动器组合 | | | 可更换风扇过滤器 | | 前置 I/O | 抗震动卡架 | | | | |  |
| *特性* | | | | | | |  |  |  |  | *尺寸 ( 单位 : mm)* | | |  |  |  |  |  |  |



● 经济实用型，符合 RoHS 标准




● 灵活的驱动器组合

● 前面板设有 2 个 USB 接口




● 12 cm 冷却风扇可简单地更换风扇过滤器



● 带锁设置防止未授权访问




*规格*



|  |  |  |
| --- | --- | --- |
| 材质 | 重型金属 |  |
| 主板规格 | 全长CPU卡 |  |
|  | 3 x 5.25” + 1 x 3.5” HDD |  |
| 驱动器组合 | or 2 x 5.25” + 2 x 3.5” HDD |  |
| or 2 x 5.25” + 1 x 3.5” HDD + 1 x front accessible |  |
|  |  |
|  | 3.5” or 2 x 5.25” + 2 x front accessible 3.5” |  |
| 散热风扇 | 1 x 12 cm |  |
| I/O 接口 | 2 x USB |  |
| I/O 开口 | 2 x COM, 2 x LPT |  |
| 扩展槽 | 14 slots for RACK-360G |  |
| 7 slots for RACK-360GATX |  |
|  |  |
| 指示灯 | Power, HDD |  |
| 按钮 | 电源开关, 重启键 |  |
| 操作温度 | 0°C ~ 50°C |  |
| 操作湿度 | 10% ~ 90% |  |
| 颜色 | B: 黑色/W: 白色 |  |
| 净重/毛重 | 11 kg/15.4 kg |  |
| 尺寸(DxWxH) | 435.5 mm x 431 mm x 176 mm |  |

*订购信息*



|  |  |  |  |
| --- | --- | --- | --- |
| 料号 |  | 描述 |  |
| RACK-360G | -R23/ACE-935AL | 4U 14-slot rackmount chassis, USB, (black/white), |  |
| with ACE-935AL-RS PSU (300W), RoHS |  |
|  |  |  |

4U 14-slot rackmount chassis, (black/white),



RACK-360G  -R23/A130B 1 x 12 cm fan, with ACE-A130B-R10 (300W ATX model), RoHS

4U ATX motherboard rackmount chassis, (black/

RACK-360G  ATX-R23/A130B white), 1 x 12 cm fan, with ACE-A130B-R10 (300W ATX model), RoHS


 颜色 Code: B-黑色 W-白色

*底板 ( 选配 )*



|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 型号 | SBC 类型 | PCI | ISA | PCIX |  | PCle |  | PSU 接口 |  |
|  |  |  |  |
| x1 | x4 | x16 |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
| PCI-13SD-RS | PICMG 1.0 | 3+4 | 3+3 | 0 | 0 | 0 | 0 | AT/ATX |  |
|  |  |  |  |  |  |  |  |  |  |
| PCI-14S2-RS | PICMG 1.0 | 4 | 8 | 0 | 0 | 0 | 0 | AT/ATX |  |
|  |  |  |  |  |  |  |  |  |  |
| PCI-14S3-RS | PICMG 1.0 | 4 | 9 | 0 | 0 | 0 | 0 | AT/ATX |  |
|  |  |  |  |  |  |  |  |  |  |
| PX-14S3-RS | PICMG 1.0 | 12 | 2 | 0 | 0 | 0 | 0 | AT/ATX |  |
|  |  |  |  |  |  |  |  |  |  |
| PX-14S5-RS | PICMG 1.0 | 7 | 6 | 0 | 0 | 0 | 0 | AT/ATX |  |
|  |  |  |  |  |  |  |  |  |  |
| BP-14S-RS | ISA | 0 | 14 | 0 | 0 | 0 | 0 | AT |  |
|  |  |  |  |  |  |  |  |  |  |
| PE-6S | PICMG 1.3 | 2 | 0 | 0 | 2 | 0 | 1 | ATX |  |
|  |  |  |  |  |  |  |  |  |  |
| PE-10S | PICMG 1.3 | 4 | 0 | 0 | 4 | 0 | 1 | ATX |  |
|  |  |  |  |  |  |  |  |  |  |
| PE-10S2 | PICMG 1.3 | 4 | 0 | 0 | 4 | 0 | 1 | ATX |  |
|  |  |  |  |  |  |  |  |  |  |
| PXE-12S | PICMG 1.3 | 4 | 0 | 6 | 0 | 0 | 1 | ATX |  |
|  |  |  |  |  |  |  |  |  |  |
| PE-13SD | PICMG 1.3 | 4 | 0 | 0 | 4 | 1 | 2 | ATX |  |
|  |  |  |  |  |  |  |  |  |  |
| PXE-13S | PICMG 1.3 | 8 | 0 | 0 | 3 | 0 | 1 | ATX |  |
|  |  |  |  |  |  |  |  |  |  |
| SPXE-14S | PICMG 1.3 | 0 | 0 | 0 | 12 | 0 | 0 | ATX |  |
|  |  |  |  |  |  |  |  |  |  |

*电源 ( 选配 )*



|  |  |  |  |
| --- | --- | --- | --- |
| 类型 | 型号 | 功率 |  |
|  |  |  |  |
| AT | ACE-935AL-RS | 300W |  |
|  |  |  |
| ACE-T140A-RS | 400W |  |
|  |  |
|  |  |  |  |
|  | ACE-A130B-R10 | 300W |  |
|  |  |  |  |
| ATX | ACE-A140A-S-R11 | 400W |  |
|  |  |  |  |
|  | ACE-A160A-R11 | 600W |  |
|  |  |  |  |
| ATX Redundant | ACE-R4130AP-RS | 300W |  |
|  |  |  |
| ACE-R4140AP-RS | 400W |  |
|  |  |
|  |  |  |  |

RACK-360G 支持单个 PS/2 PSU。想了解威强电更多的电源产品，请参考章节 5 或直接访问 www.ieiworld.com.cn



RACK-360G-2019-V10